**How to program Genway Direct Calling Cat-5 Apt Door Stations**

**NB - You only need to do this if you have messed about with the pre-programmed settings already. The unit comes from the factory with the buttons already set up. If you plug everything in, it should just work**

Connect all the pieces of kit as per the instructions

Set the 4110 Distributor Dip switch to the correct setting: Dip switch 1 ON, all the others OFF

1. To log into the Programmable Doorstation, key in on the remote:

FN (function)

1234 (the default password)

ENTER

2. You are going to set the Programmable doorstation as Doorstation one, and the distributor as distributor one. To set these Programmable Doorstation parameters, key in:

SERVICE

UNLOCK

0001

1

ENTER

Now press EXIT twice.

3. Next, you are going to set up the individual monitors in the Programmable doorstation. First repeat step 1 to log in. To set the individual monitor parameters, key into the remote:

FN (function)

REG-

Now press the BUTTON on the Doorstation you wish to set up. I usually start with the top button.

0001 (this is the first monitor)

001 (this is the distributor number, always 001)

1 (port number. Check on the 4110 distributor to see which port is the first one)

ENTER

You have now set up the first monitor. Now to set up the second one. Press the second button on the doorstation. Now key into the remote:

0002 (this is the second monitor)

001

2 (port two)

ENTER

You have now set the second monitor. Repeat the process for the third monitor. Press the third button on the doorstation. Now key into the remote:

0003 (this is the third monitor)

001

3 (port three)

ENTER

You have now set the third monitor. Repeat the process for the fourth monitor. Press the fourth button on the doorstation. Now key into the remote:

0004 (this is the fourth monitor)

001

4 (port four)

ENTER

You are now finished setting up the monitors.

4. What should you do if one of the monitor programming sequences goes wrong? Quite often when setting up these systems, instead of hearing the long SUCCESS beep, you will hear BEEP BEEP BEEP and possibly ‘Sorry, wrong number’ from the womans voice. Here is what to do.

First, hit EXIT on the remote TWICE

Second, unplug the power lead to reset the system

Third, log on to the Programmable doorstation using STEP 1 above

Fourth, press FN then REG- on the remote

Fifth, press the doorbell BUTTON which didn’t respond properly the first time

Sixth, repeat the input of the info which corresponds to that BUTTON. Lets use BUTTON three as an example:

0003 (this is the third monitor)

001

3 (port three)

ENTER

Listen for the long BEEP which tells you the programming was successful. Repeat this process for all buttons which didn’t respond properly the first time.

Once you have finished all programming, power off the system, and power it back on. Press all the buttons on the doorstation in sequence to check to make sure they work.

Have a nice day.