T-Views Installation and Usage Manual

Downloading
1. Click on the link to the T-Views Photo Software
2. Save the RAR file to your computer
3. Use either WinRAR or Winzip to un-compress the installation file, t-views-photo-setup.exe 
4. Make a note of where you saved the installation file

Installation
1. Double click on the file, t-views-photo-setup.exe
2. Do not install to the C:\Program Files\TViews\ folder. You need to install the program to a drive other than C:\
3. You can install the program to any other drive, even a USB drive. You cannot install to the CD drive.
4. If asked, give your computer permission to install the software.

Running the software
1. The installation has installed two programs to your computer- T-Views Album, and T-Views Memo
2. First, open T-Views Album. Now, open T-Views Memo
3. There are four buttons along the top- Import Pictures, Copy All to SD, Setting, and Help
4. You will only need the first three. Help is completely useless.
5. Under the buttons you will see 'Scaling Mode'. There are three modes, Normal, Cropping and Full
6. Our testing has shown that Cropping is most likely to give you a good picture. Normal will leave blank spaces at the sides of the picture, and Full distorts pictures quite often
7. So, once you have clicked on 'Cropping', click on the button 'Import Pictures'
8. Select the pictures you wish to see via your Door Entry Monitor. You can select up to 800. You may need to change directories to see your pictures
9. Once you have selected the pictures, click 'Open'
10. All of your pictures will be converted into a file format called TVS. This is the format your Door Entry Monitor understands.
11. Once the pictures have been converted, you can check through to make sure you picked the right ones
12. Now you have checked the pictures, you can copy them to your SD card by clicking  'Copy All to SD'
13. Please note, Your SD card must be connected to your PC either through a built-in SD card reader, or a USB card reader device
14. Now that the TVS format photos are on the SD card, you can see them using T-Views Memo
15. Make sure that the photos are in a folder called ALBUM. If they are not, the monitor will not be able to see them
16. You can now remove the SD card from the reader and place it in the monitor